{"text_format":"3","workbook":"xls","n_sheets":2,"sheets":["主要跨界河流简评","重污染河流简评"],"not_rendered":{"external_links":1,"defined_names":3,"comments":1},"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"主要跨界河流简评","index":0,"n_rows":7,"n_cols":11,"rows_kept":7,"merged":[[0,0,0,10],[2,0,3,0],[6,0,9,10]],"flags":["formulas_cached_only"]}
["2016年8月份广东省主要跨市河流交接断面水质状况"]
["责任\n城市","监测城市","交接断面","所在河流","交接关系","水质控\n制目标","水质\n类别","上年同期\n水质类别","达标\n状况","主要超标项目\n/超标倍数","备注"]
["深圳","惠州","西湖村","龙岗河","深圳→惠州","Ⅲ","劣V","劣V","超标","氨氮/1.1，总磷/1.1","2016年，氨氮低于3mg/L，总磷低于0.35mg/L，其他指标达Ⅳ类。"]
[null,"惠州","上垟","坪山河","深圳→惠州","Ⅲ","劣V","劣V","超标","总磷/1.4，氨氮/0.2","2016年，氨氮低于2.5mg/L，其他指标达Ⅳ类。"]
["河源","惠州","江口","东江","河源→惠州","Ⅱ","Ⅱ","Ⅱ","达标","—"]
["东莞","惠州","石龙桥(左)","东江","惠州→东莞共河","Ⅱ","Ⅲ","Ⅱ","超标","总磷/0.7，氨氮/0.4，溶解氧/0.9"]
["备注：1.未监测统一用长划号填写；\n      2.超标项目/超标倍数计算，溶解氧为目标浓度与监测浓度的差值，其他指标以阶段目标计算，无阶段目标的以水质目标计算;\n      3.综合污染指数计算指标为《国家地表水标准2002-3838》表1中的除水温、总氮、粪大肠菌群、pH、溶解氧外的19项指标。"]

{"sheet":"重污染河流简评","index":1,"n_rows":9,"n_cols":20,"rows_kept":9,"merged":[[0,0,0,12],[1,0,2,0],[1,1,2,1],[1,2,2,2],[1,3,2,3],[1,4,2,4],[1,5,2,5],[1,6,2,6],[1,7,2,7],[1,8,2,8],[1,9,2,9],[1,10,1,11],[1,12,2,12],[6,0,8,12]],"flags":["formulas_cached_only"]}
["2016年8月份重污染河流断面水质状况"]
["责任城市","监测城市","河流\n名称","断面\n名称","水质\n目标","水质\n类别","水质\n状况（手工）","达标\n状况","超标项目\n/超标倍数","各指标与上年同期比较","综合污染指数",null,"备注"]
[{"$nulls":10},"2016-08-01","与上年\n同期比较"]
["深圳","惠州","龙岗河","西湖村","Ⅲ","劣V","重度污染","超标","氨氮/1.1，总磷/1.1","总磷/20.0%、氨氮/3.5%、化学需氧量/-30.4%、溶解氧/-17.3%",{"v":3.546666666666667,"d":"3.55"},{"v":0.045,"d":"4.5%"},"2016年，氨氮低于3mg/L，总磷低于0.35mg/L，其他指标达Ⅳ类。"]
["深圳","惠州","坪山河","上垟","Ⅲ","劣V","重度污染","超标","总磷/1.4，氨氮/0.2","氨氮/27.2%、化学需氧量/0.0%、总磷/67.4%、溶解氧/-40.3%",2.59,{"v":0.375,"d":"37.5%"},"2016年，氨氮低于2.5mg/L，其他指标达Ⅳ类。"]
["惠州","惠州","淡水河","紫溪","Ⅲ","劣V","重度污染","超标","氨氮/0.3，总磷/0.2","总磷/127.8%、氨氮/-26.4%、化学需氧量/-33.3%、溶解氧/-12.6%",{"v":2.1733333333333333,"d":"2.17"},{"v":-0.078,"d":"-7.8%"},"2016年，氨氮低于3mg/L，总磷低于0.35mg/L，其他指标达Ⅳ类。",{"$nulls":6},"     "]
["备注：1.未监测统一用长划号填写；\n      2.超标项目/超标倍数计算，溶解氧为目标浓度与监测浓度的差值，其他指标以阶段目标计算，无阶段目标的以水质目标计算;\n      3.综合污染指数以氨氮、总磷和化学需氧量三项计算。\n      4.镇盛无2015年阶段目标，参照下游石碧阶段目标；水口水道沿用2014年阶段目标。"]
[]
[{"$nulls":19},"     "]